|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| https://www-p.unisa.edu.au/styleguide/logos/images/logo_unisa_RGB-blue.png | WHS FORM | | ELECTRICAL EQUIPMENT REGISTER | | | | | | | | | | **WHS25** | |
|  | | *Including Portable RCDs - tested using the RCD test button observing that the operating time is ‘without undue delay’.*  *It is the responsibility of the unit/institute to perform testing on any RCD which is not in an FMU-controlled distribution board or cupboard.*  This form supports the ***In-service inspection and testing of electrical equipment*** procedure | | | | | | | | | |  | |
| **Workplace:** | | | | | | | | | | | | | | |
| **Plant ID No or Item No:** | | **Description of electrical equipment**  **(including serial number if applicable)** | | **Building/ Level eg**  **IW2** | **Room no/location eg IW2-02 or IW2 kitchen** | **Class** | **Test freq.** | **Date tested** | **Result Passed/ Failed** | **Name of competent person** | **Action taken if Failed** | **Record of repairs** | | **Date next test due** |
| 1017 | | Gilson p-pump | | H2 | H2-03 workshop | 1 | 12 | 15/8/2014 | Pass | F Smith | - | - | | 15/8/2015 |
|  | |  | |  |  |  |  |  |  |  |  |  | |  |
|  | |  | |  |  |  |  |  |  |  |  |  | |  |
|  | |  | |  |  |  |  |  |  |  |  |  | |  |
|  | |  | |  |  |  |  |  |  |  |  |  | |  |
|  | |  | |  |  |  |  |  |  |  |  |  | |  |
|  | |  | |  |  |  |  |  |  |  |  |  | |  |
|  | |  | |  |  |  |  |  |  |  |  |  | |  |
|  | |  | |  |  |  |  |  |  |  |  |  | |  |
|  | |  | |  |  |  |  |  |  |  |  |  | |  |
|  | |  | |  |  |  |  |  |  |  |  |  | |  |

|  |  |  |
| --- | --- | --- |
| **Class** | **Test frequency** | **Result:** |
| I - protectively earthed  II - double insulated  EPOD  PRCD - portable RCD  NPRCD - non-portable RCD  Cord set  Cord extension set | 6 - 6 monthly  12 - annually  60 - 5-yearly  NT - Not tested based on assessment | Pass  Fail  Removed  Unavailable |

**Legend:**